New USB-C panel mount jacks

Georg Schlegel GmbH & Co. KG expands its panel mount jack range by two additional USB-C versions.

The usage of USB-C devices in the industrial sector is increasing steadily. So, Schlegel's contribution to this trend are two new USB-C panel mount jacks. Both jacks are designed as USB-C jacks on the front side.

The jack RRJ\_USB\_CA\_60 has a 60 cm cable and a USB type A connector on the rear side, and therefore can be connected to devices having conventional USB-A connectors. The jack RRJ\_USB\_CC\_60 also has a 60 cm cable on the rear side, but with a USB type C connector to connect two USB-C interfaces. Both versions support USB 2.0.

The USB-C panel mount jacks are available with silver-coloured, black or stainless steel front bezel.

